{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["LEACH PCB Breakout"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"LEACH PCB Breakout","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Reference"," Quantity"," Value"," Footprint","Part Number","Additional Part"]
["J3 J4 J5 J6 J7 J8 ",6,"1x3_Header","Jumper3_050","S9016E-03-ND ","952-1727-ND"]
["P1 ",1,"DB-50_FEMALE","DB50_173-50FEA","A32159-ND"]
["P2 ",1,"DB-37_MALE","DB37M-A-DS37AKG","AE10988-ND"]
["P3 ",1,"DB-25_FEMALE","DB25F-A-DF25AKG","AE10937-ND"]
["P4 P5 ",2,"DB-15_MALE","DB15M-ADS15A-KG-TAXB5","AE10977-ND "]
["P6 P9 P7 P8 ",4,"SMA","SMA","A97594-ND"]