{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Bill of Materials"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Bill of Materials","index":0,"n_rows":56,"n_cols":12,"rows_kept":56,"cut":false,"hidden":false,"merged":[[1,8,3,11]],"flags":["formulas_cached_only"]}
["Bill of Materials"]
["System:",null,"DAMIC-M Frontend Board (based on ADA4817), MK2",null,"Source Data From:","FE_ADA4817_MK2.PrjPcb",null,null,"Physik Institut\nUniversitaet Zuerich       Winterthurerstrasse 190, CH-8057 Zuerich"]
["Board:",null,"FE_ADA4817_MK2",null,"Project:","FE_ADA4817_MK2.PrjPcb"]
["Board Revision:",null,"1.1",null,"Variant:","None"]
[]
["#","Designator","Part Description","Part Number","Value","Type","Specific","Footprint","Manufacturer","Distributor","Distributor Part Number","Quantity"]
[1,"C210, C211, C212, C213, C214, C215, C224, C225","Capacitor Ceramic","CGA3E2X7R1H473K080AA","47n","CAP CER 0.047UF 50V X7R 0603","-",603,"TDK","Digikey","445-5664-1-ND",8]
[2,"C216, C217, C218, C219, C220, C221","Capacitor Ceramic","CGA3E2X7R1H223K080AA","22n","CAP CER 0.022UF 50V X7R 0603","-",603,"TDK","Digikey","445-5663-1-ND",6]
[3,"C222, C223, C226, C227, C228, C229, C230, C231","Capacitor Ceramic","C1608NP01H331J080AA","330p","CAP CER 330PF 50V NP0 0603","-",603,"TDK","Digikey","445-14075-1-ND",8]
[4,"C240","Capacitor Ceramic","C4532X7T2E105K250KE","1u","CAP CER 1UF 250V X7T 1812","-","1812_2","TDK","Digikey","445-8874-1-ND",1]
[5,"C241","Capacitor Ceramic","C3216C0G2E103J115AA","10n","CAP CER 10000PF 250V C0G 1206","-",1206,"TDK","Digikey","445-15417-1-ND",1]
[6,"C242, C245","Capacitor Ceramic","C3216X5R1E336M160AC","33u","CAP CER 33UF 25V X5R 1206","-",1206,"TDK","Digikey","445-8046-1-ND",2]
[7,"C243, C246, C255, C258","Capacitor Ceramic","C1608X5R1E475K080AC","4u7","CAP CER 4.7UF 25V X5R 0603","-",603,"TDK","Digikey","445-9050-1-ND",4]
[8,"C244, C247, C250, C253, C256, C259, C303, C304, C313, C314, C323, C324, C333, C334, C343, C344, C353, C354, C363, C364, C373, C374","Capacitor Ceramic","CGA3EAC0G2A103J080AC","10n","CAP CER 10000PF 100V C0G 0603","-",603,"TDK","Digikey","445-16158-1-ND",22]
[9,"C248, C251, C254, C257","Capacitor Ceramic","C2012X5R1E156M125AC","15u","CAP CER 15UF 25V X5R 0805","-",805,"TDK","Digikey","445-9078-1-ND",4]
[10,"C249, C252","Capacitor Ceramic","C1608X5R1E225K080AB","2u2","CAP CER 2.2UF 25V X5R 0603","-",603,"TDK","Digikey","445-5964-1-ND",2]
[11,"C260","Capacitor Ceramic","CC0805KKX7RYBB104","100n","CAP CER 0.1UF 250V X7R 0805","-",805,"YAGEO","Digikey","13-CC0805KKX7RYBB104CT-ND",1]
[12,"C270, C275","Capacitor Aluminum","-","OPEN","CAP ALUM SMD OPEN","6.6 x 6.6 x 6mm, optional Panasonic EEE-FN1A221UP","CASE_FK_D_H6_STEP","-","-","-",2]
[13,"C300, C307, C312, C315, C317, C319, C320, C327, C332, C335, C337, C339, C340, C347, C352, C355, C357, C359, C360, C367, C372, C375, C377, C379","Capacitor Ceramic","C1608X7R1H104K080AA","100n","CAP CER 0.1UF 50V X7R 0603","-",603,"TDK","Digikey","445-1314-1-ND",24]
[14,"C301, C321, C341, C361","Capacitor Ceramic","CGA3E2C0G1H100D080AA","10p","CAP CER 10PF 50V C0G 0603","-",603,"TDK","Digikey","445-5628-1-ND",4]
[15,"C302, C305, C322, C325, C342, C345, C362, C365","Capacitor Ceramic","CGA3E1X7R1V105K080AC","1u","CAP CER 1UF 35V X7R 0603","-",603,"TDK","Digikey","445-174215-1-ND",8]
[16,"C316, C318, C336, C338, C356, C358, C376, C378","Capacitor Ceramic","GRM188D71A106MA73D","10u","CAP CER 10UF 10V X7T 0603","4uF typ @ 5V, 6uF typ @ 3.3V",603,"Murata","Digikey","490-7200-1-ND",8]
[17,"C380, C381, C385, C386","Capacitor Ceramic","GRM31CC81E226ME11L","22u","CAP CER 22UF 25V X6S 1206","-",1206,"Murata","Digikey","490-16314-1-ND",4]
[18,"CON200","Connector 2 x 30 contacts plus shield connections","ERF8-030-05.0-L-DV-L-K-TR; additional standoffs, 2x SO-0600-01-01-01-N","ERF8-030-05.0-L-DV-L-K-TR","CONN SOCKET 60POS SMD GOLD","Female","SAMTEC_ERF8-030-05.0-L-DV-L-TR_SO_6","Samtec","Digikey","SAM13578CT-ND; order also 2x 612-SO-0600-01-01-01-N-ND",1]
[19,"CON240","Connector 2 x 30 contacts plus shield connections","ERM8-030-01-L-D-EM2-L-TR","ERM8-030-01-L-D-EM2-L-TR","CONN HDR 60POS EDGE MNT GOLD","Male","SAMTEC_ERM8-030-01-X-D-EM2-L-TR","Samtec","Digikey","SAM13749CT-ND",1]
[20,"D385","Diode Zener","BZX38450-C1V8F","1V8","BZX38450-C1V8/SOD323/SOD2","-","SOD-323F","Nexperia","Digikey","1727-BZX38450-C1V8XCT-ND",1]
[21,"D390, D391","LED","APT1608LSYCK/J3-PRV","APT1608LSYCK/J3-PRV","LED YELLOW CLEAR 2SMD","1.85V, 25mcd @ 2mA","0603 LED 2","Kingbright","Digikey","754-1932-1-ND",2]
[22,"FID200, FID201, FID202","Fiducial on PCB","-","Fiducial","-","Not equipped (part of PCB)","FIDUCIAL_1MM","-","-","-",3]
[23,"JP200","Unshrouded Header","75160-101-02LF","75160-101-02LF","CONN HEADER VERT 2POS 2.54MM","-","SIP1x2_STEP","FCI","Digikey","609-75160-101-02LF-ND; order also S9001-ND",1]
[24,"R200, R280, R281","Chip Resistor","CRCW06030000Z0EAC  ","0R","RES 0 OHM JUMPER 1/10W 0603  ","-",603,"Vishay, Vishay  ","Digikey","541-4012-1-ND  , 541-4012-1-ND",3]
[25,"R210, R211, R212, R213, R214, R215, R224, R225","Chip Resistor","CRCW0603200RFKEAC","200R","RES 200 OHM 1% 1/10W 0603","-",603,"Vishay Dale","Digikey","541-4035-1-ND",8]
[26,"R216, R217, R218, R219, R220, R221","Chip Resistor","CRCW0603470RFKEAC","470R","RES 470 OHM 1% 1/10W 0603","-",603,"Vishay Dale","Digikey","541-4038-1-ND",6]
[27,"R222, R223, R226, R227, R228, R229, R230, R231","Chip Resistor","CRCW0603100RFKEAC","100R","RES 100 OHM 1% 1/10W 0603","-",603,"Vishay Dale","Digikey","541-3951-1-ND",8]
[28,"R240","Chip Resistor","-","OPEN","RES SMD OPEN 0805","-",805,"-","-","-",1]
[29,"R242, R245, R248, R251, R254, R257, R301, R321, R341, R361","Chip Resistor","CRCW0603100KFKEAC","100k","RES 100K OHM 1% 1/10W 0603","-",603,"Vishay Dale","Digikey","541-3950-1-ND",10]
[30,"R260","Chip Resistor","KTR10EZPF3904","3M9","RES SMD 3.9M OHM 1% 1/8W 0805","400V, ±100ppm/K",805,"Rohm","Digikey","RHM3.9MAHCT-ND",1]
[31,"R300, R320, R340, R360","Chip Resistor","CRCW060320K0FKEAC","20k","RES 20K OHM 1% 1/10W 0603","-",603,"Vishay Dale","Digikey","541-3987-1-ND",4]
[32,"R302, R322, R342, R362","Chip Resistor","RR0816Q-910-D","91R","RES SMD 91 OHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08Q91DCT-ND",4]
[33,"R303, R323, R343, R363","Chip Resistor","RR0816P-1151-D-07H","1k15","RES SMD 1.15KOHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08P1.15KDCT-ND",4]
[34,"R311, R331, R351, R371","Chip Resistor","CRCW06030000Z0EAC","0R","RES 0 OHM JUMPER 1/10W 0603","-",603,"Vishay","Digikey","541-4012-1-ND",4]
[35,"R312, R314, R332, R334, R352, R354, R372, R374","Chip Resistor","RT0603DRD07249RL","249R","RES SMD 249 OHM 0.5% 1/10W 0603","Thin Film",603,"YAGEO","Digikey","YAG4799CT-ND",8]
[36,"R313, R315, R333, R335, R353, R355, R373, R375","Chip Resistor","RT0603DRE07499RL","499R","RES SMD 499 OHM 0.5% 1/10W 0603","Thin Film",603,"YAGEO","Digikey","311-2596-1-ND",8]
[37,"R316, R317, R336, R337, R356, R357, R376, R377","Chip Resistor","RR0816Q-510-D","51R","RES SMD 51 OHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08Q51DCT-ND",8]
[38,"R380","Chip Resistor","RR0816P-102-D","1k","RES SMD 1K OHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08P1.0KDCT-ND",1]
[39,"R381","Chip Resistor","RR0816P-472-D","4k7","RES SMD 4.7K OHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08P4.7KDCT-ND",1]
[40,"R385","Chip Resistor","AC0603FR-073K9L","3k9","RES SMD 3.9K OHM 1% 1/10W 0603","-",603,"Yageo","Digikey","YAG3606CT-ND",1]
[41,"R386","Chip Resistor","RR0816P-362-D","3k6","RES SMD 3.6K OHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08P3.6KDCT-ND",1]
[42,"R387","Chip Resistor","RR0816P-162-D","1k6","RES SMD 1.6K OHM 0.5% 1/16W 0603","Thin Film",603,"Susumu","Digikey","RR08P1.6KDCT-ND",1]
[43,"R390, R391","Chip Resistor","CRCW06031K00FKEAHP","1k","RES SMD 1K OHM 1% 1/3W 0603","-",603,"Vishay Dale","Digikey","541-1.00KSCT-ND",2]
[44,"SH380","RF Shield","MS520-10F","MS520-10","RF SHLD FRAME 1.051\"X2.047\" SLDR","52mm x 26.7mm x 6mm","RF_SHIELD_MS520-10F_MODI_TO","Masach Tech Ltd.","Digikey","2333-MS520-10F-ND; order also 2333-MS520-10C-ND",1]
[45,"TP200","Testpoint",5001,"-","PC TEST POINT MINIATURE BLACK","Pad 1 / 1.6mm","TP_THT_KEYSTONE_5001","Keystone","Digikey","36-5001-ND",1]
[46,"U300, U320, U340, U360","Low Noise FastFET OpAmp","ADA4817-1ARDZ-R7","ADA4817-1ARDZ","IC VOLTAGE FEEDBACK 1 CIRC 8SOIC","-","SO8_EP","AD","Digikey","505-ADA4817-1ARDZ-R7CT-ND",4]
[47,"U310, U330, U350, U370","Low Power, Differential ADC Driver","ADA4945-1ACPZ-R7","ADA4945-1","IC ADC DRIVER 16LFCSP","-","QFN50P300X300X100-17CN","AD","Digikey","505-ADA4945-1ACPZ-R7CT-ND",4]
[48,"U380","Positive Voltage Regulator, Low Noise","ADP7118AUJZ-3.3-R7","ADP7118-3.3","IC REG LIN 3.3V 200MA TSOT23-5","20 VIN max.","SOT23-5","AD","Digikey","505-ADP7118AUJZ-3.3-R7CT-ND",1]
[49,"U385","Negative Voltage Regulator, Low Noise","ADP7182AUJZ-R7","ADP7182","IC REG LIN NEG ADJ 200MA TSOT23","-28 VIN max.","SOT23-5","AD","Digikey","505-ADP7182AUJZ-R7CT-ND",1]
[{"$nulls":10},"Total Quantity","214"]